-----------------------------------------------------------------------------------

--------------------------------------------------------

 4.2.7 Build 116 - 21.12.2020

-----------------------------------------------------------------------------------

--------------------------------------------------------

Inverters/SCBs/meters/battery systems/other devices:

New:

Extensions:

- Delta Sunspec: Delta RPI M70A.

Adjustments:

- Growatt Max: Prioritization of error messages changed

Bug fixes:

- Keba: Sometimes only one third of the possible power was loaded. Fixed.

- Huawei V2: With FW 4.2.7 Build 116, UDC was recorded incorrectly when both trackers were occupied. Fixed.

- Kaco blueplanet 87.0 – 150 TL3: Yield value was not recorded correctly. Fixed.

- Detection of Aros 485, Aros 422 and Riello works again.

- Azzurro: Detection sometimes resulted in wrong tracker count and incorrect data. Fixed.

- SMA Modbus: System password could not be configured. Fixed.

Extensions:
Adjustments:
Bug fixes:
- Calculation of fixed CosPhi values on master/slave systems corrected.