-----------------------------------------------------------------------------------

--------------------------------------------------------

 4.2.7 Build 116 Beta - 26.03.2021

-----------------------------------------------------------------------------------

--------------------------------------------------------

Inverters/SCBs/meters/battery systems/other devices:

New:

Extensions:

- Delta Sunspec: Delta RPI M70A.

 - Sungrow: New models:

 SG8KTL-M,SG10KTL-M,SG12KTL-M,SG15KTL-M,SG17KTL-M,SG20KTL-M,SG30KTL-M,SG36KTL-M,SG50KTL-M-20,SG30KTL-M-V31,

SG5KTL-MT,SG6KTL-MT,SG10KTL-MT,SG111HV,SG125HV,SG125HV-20, SG33K3J

Adjustments:

 - Growatt Max: Prioritization of error messages changed

Bug fixes:

- Keba: Sometimes only one third of the possible power was loaded. Fixed.

- Huawei V2: With FW 4.2.7 Build 116 UDC was recorded incorrectly when both trackers were occupied. Fixed.

- Kaco blueplanet 87.0 – 150 TL3: Yield value was not recorded correctly. Fixed.

- Detection of Aros 485, Aros 422 and Riello works again.

- Azzurro: Detection sometimes resulted in wrong tracker count and incorrect data. Fixed.

- SMA Modbus: System password could not be configured. Fixed.

- SMA Core1: Plant password could only contain digits.

Extensions:
Adjustments:
Bug fixes:
- Calculation of fixed CosPhi values on master/slave systems corrected.